**Potential hazards of confined spaces:**



* Toxic fumes
* Oxygen deficiency
* Explosive atmosphere
* Exposure to hazardous energies
* Moving machine parts
* Engulfment/entrapment

**Safety precautions:**

* **Perform a hazard assessment:** Identify all hazards and needed controls. Include hazards created by the work itself.
* **Get a confined space permit signed by a confined space entry supervisor**.
* **Monitor air:**
* Provide initial and continuous monitoring for toxics, flammables, and oxygen.
* Ventilate and monitor when performing hot work or applying chemicals either in a confined space or an adjacent area.
* Check for adequate, continuous ventilation when hazardous atmospheres are possible.
* **Lock-out all energy sources:** This includes stored energies.
* **Use proper controls and protective equipment:** This includes respiratory, skin, eye, and fall protection.
* **Set up a retrieval device.**



* **Confirm that training is current** **for:**
* Entry personnel
* Attendants
* Supervisors
* Rescue personnel
* **Ensure that rescue personnel are available.**
* **Ensure that the attendant is:**
* At the point of entry.
* In communication with rescue and entry personnel.
* **Know how to prevent heat stress:**
* Take breaks as needed in a cool environment.
* Drink fluids.

This form documents that the training specified above was presented to the listed participants. By signing below, each participant acknowledges receiving this training.

Organization: Date:

Trainer: Trainer’s Signature:

**Class Participants:**

Name: Signature:

Name: Signature:

Name: Signature:

Name: Signature:

Name: Signature:

Name: Signature:

Name: Signature:

Name: Signature:

Name: Signature:

Name: Signature:

Name: Signature:

Name: Signature:

Name: Signature:

Name: Signature:

Name: Signature:

Name: Signature: